//
//			Version R01			2013/09/04
//
// =============================================================================
// The RTK channel plan Rule
//
// You need to use RT channel plan to update in below country. And select what
// you need in proper field.
// Please refer to document.EFSUE channel plan filed. Now the definition
// is from 0x20 ~ 0x53 in R07 version, and corresponding EFSUE data sheet.
// But for EFUSE and driver known channel plan mapping.Plese use  
// 
//
// =============================================================================
// Channel Plan Contents				
// Domain 		Code			EEPROM			RegistryChannelPlan
// 2G RD		5G RD			Bit[6:0]		Decimal
//
// 2G_WORLD		5G_NULL			20h				25
// 2G_ETSI1		5G_NULL			21h				26
// 2G_FCC1		5G_NULL			22h				27
// 2G_MKK1		5G_NULL			23h				28
// 2G_ETSI2		5G_NULL			24h				29
// 2G_FCC1		5G_FCC1			25h				30
// 2G_WORLD		5G_ETSI1		26h				31
// 2G_MKK1		5G_MKK1			27h				32
// 2G_WORLD		5G_KCC1			28h				33
// 2G_WORLD		5G_FCC2			29h				34
// 2G_WORLD		5G_FCC3			30h				35
// 2G_WORLD		5G_FCC4			31h				36
// 2G_WORLD		5G_FCC5			32h				37
// 2G_WORLD		5G_FCC6			33h				38
// 2G_FCC1		5G_FCC7			34h				39
// 2G_WORLD		5G_ETSI2		35h				40
// 2G_WORLD		5G_ETSI3		36h				41
// 2G_MKK1		5G_MKK2			37h				42
// 2G_MKK1		5G_MKK3			38h				43
// 2G_FCC1		5G_NCC1			39h				44
// 2G_FCC1		5G_NCC2			40h				45
// 2G_Global	5G_NULL			41h				46
// 2G_ETSI1		5G_ETSI4		42h				47
// 2G_FCC1		5G_FCC2			43h				48
// 2G_FCC1		5G_NCC3			44h				49
// 2G_WORLD		5G_ETSI5		45h				50
// 2G_FCC1		5G_FCC8			46h				51
// 2G_WORLD		5G_ETSI6		47h				52
// 2G_WORLD		5G_ETSI7		48h				53
// 2G_WORLD		5G_ETSI8		49h				54
// 2G_WORLD		5G_ETSI9		50h				55
// 2G_WORLD		5G_ETSI10		51h				56
// 2G_WORLD		5G_ETSI11		52h				57
// 2G_FCC1		5G_NCC4			53h				58
// 2G_WORLD     5G_ETSI12       54h             59
// 2G_FCC1      5G_FCC9         55h             60
// 2G_WORLD     5G_ETSI13       56h             61
// 2G_FCC1      5G_FCC10        57h             62
// 2G_MKK2		5G_MKK4			58h				63
// 
// =============================================================================
// 2.4G Regulatory Domains				
// 2G RD		Regulation		Channels
//
// 2G_WORLD		ETSI			1~13
// 2G_ETSI1		ETSI			1~13
// 2G_FCC1		FCC				1~11
// 2G_MKK1		MKK				1~13, 14
// 2G_MKK2		MKK				1~13
// 2G_ETSI2		ETSI			10~13
// 2G_Global	ETSI			1~13, 14
//
//
// =============================================================================
// 5G Regulatory Domains				
// 5G RD		Regulation		Channels							Frequencyes	Note
//
// 5G_NULL		NA				NA									NA
// 5G_ETSI1		ETSI			36~48, 52~64, 100~140
// 5G_ETSI2		ETSI			36~48, 52~64, 100~140, 149~165
// 5G_ETSI3		ETSI			36~48, 52~64, 100~132, 149~165
// 5G_FCC1		FCC				36~48, 52~64, 100~140, 149~165
// 5G_FCC2		FCC				36~48, 149~165
// 5G_FCC3		FCC				36~48, 52~64, 149~165
// 5G_FCC4		FCC				36~48, 52~64, 149~161
// 5G_FCC5		FCC				149~165
// 5G_FCC6		FCC				36~48, 52~64
// 5G_FCC7		FCC				36~48, 52~64, 100~116, 132~140, 149~165
// 5G_IC1		IC				36~48, 52~64, 100~116, 132~140, 149~165
// 5G_KCC1		KCC				36~48, 52~64, 100~124, 149~161
// 5G_MKK1		MKK				36~48, 52~64, 100~140
// 5G_MKK2		MKK				36~48, 52~64
// 5G_MKK3		MKK				100~140
// 5G_MKK4		MKK				36~48
// 5G_NCC1		NCC				56~64, 100~116, 132~140, 149~165
// 5G_NCC2		NCC				56~64, 149~165
// 5G_NCC3		NCC				149~165
// 5G_ETSI4		ETSI			36~48
// 5G_ETSI5		ETSI			36~48, 52~64, 100~116, 132~140, 149~165"
// 5G_FCC8		FCC				149~161
// 5G_ETSI6		ETSI			36~48, 52~64
// 5G_ETSI7		ETSI			36~48, 52~64, 149~165
// 5G_ETSI8		ETSI			36~48, 149~165
// 5G_ETSI9		ETSI			100~140
// 5G_ETSI10	ETSI			149~165
// 5G_ETSI11	ETSI			36~48, 52~64, 132~140, 149~165
// 5G_NCC4		NCC				52~64, 100~116, 132~140, 149~165
// 5G_ETSI12    ETSI            149~161
// 5G_FCC9      FCC             36~48, 100~116, 132~140, 149~165
// 5G_ETSI13    ETSI            36~48, 100~116, 132~140
// 5G_FCC10     FCC             36~48, 100~116, 132~140, 149~161
//
// =============================================================================
// SystemInfo (For user to select)
//		LOCALE_SYSTEM_DEFAULT: Get region from Windows LOCALE_SYSTEM_DEFAULT
//		LOCALE_USER_DEFAULT: Get region from Windows LOCALE_USER_DEFAULT
//
//		For example:
// 		You can select CN for XP/ and CHN for OS after Vista.
//
//		[Locale Short Name]: Set CountryRegion directly. (USA/US for example) 
//
SystemInfo=LOCALE_SYSTEM_DEFAULT
// OsVersion=
   
//
// Country compatiable.
//
[Country_Channel_Plan]
// [country code] = [channel plan]
AR=62	
// Argentina				57h
BO=35	
// Bolivia					30h
BR=39	
// Brazil					34h
CL=35
// Chile					30h
CO=39
// Colombia					34h
CR=39
// Costa Rica				34h
EC=39
// Ecuador					34h
SV=35
// El Salvador				30h
GT=39
// Guatemala				34h
HN=37
// Honduras					32h
MX=39
// Mexico					34h
NI=39
// Nicaragua				34h
PA=39
// Panama					34h
PY=39
// Paraguay					34h
PE=39
// Peru						34h
US=39
// United States			34h
UY=39
// Uruguay					34h
VE=35
// Venezuela				30h
PR=39
// Puerto Rico				34h
DO=39
// Dominican Republic		34h
AT=31
// Austria					26h
BE=31
// Belgium					26h
CY=31
// Cyprus					26h
CZ=31
// Czech Republic			26h
DK=31
// Denmark					26h
EE=31
// Estonia					26h
FI=31
// Finland					26h
FR=31
// France					26h
DE=31
// Germany					26h
GR=31
// Greece					26h
HU=31
// Hungary					26h
IS=31
// Iceland					26h
IE=31
// Ireland					26h
IT=31
// Italy					26h
LV=31
// Latvia					26h
LI=31
// Liechtenstein			26h
LT=31
// Lithuania				26h
LU=31
// Luxembourg				26h
MT=31
// Malta					26h
MC=31
// Monaco					26h
NL=31
// Netherlands				26h
NO=31
// Norway					26h
PL=31
// Poland					26h
PT=31
// Portugal					26h
SK=31
// Slovakia					26h
SI=31
// Slovenia					26h
ES=31
// Spain					26h
SE=31
// Sweden					26h
CH=31
// Switzerland				26h
GB=31
// Great Britain			26h
AL=31
// Albania					26h
AZ=31
// Azerbaijan				26h
BH=52
// Bahrain					47h
BA=31
// Bosnia & Herzegovina		26h
BG=31
// Bulgaria					26h
HR=31
// Croatia					26h
EG=52
// Egypt					47h
GH=31	
// Ghana					26h
IQ=31
// Iraq						26h
IL=52
// Israel					47h
JO=54
// Jordan					49h
KZ=31
// Kazakhstan				26h
KE=52
// Kenya					47h
KW=52
// Kuwait					47h
KG=31
// Kyrgyzstan				26h
LB=31
// Lebanon					26h
LS=31
// Lesotho					26h
MK=31
// Republic of Macedonia	26h
MA=52
// Morocco					47h
MZ=31
// Mozambique				26h
NA=31
// Namibia					26h
NG=55
// Nigeria					50h
OM=31
// Oman						26h
QA=56
// Qatar					51h
RO=31
// Romania					26h
RU=52
// Russian, gost			36h
SA=31
// Saudi Arabia				26h
SN=31
// Senegal					26h
RS=31
// Serbia					26h
ME=31
// Montenegro				26h
ZA=31
// South Africa				26h
TR=31
// Turkey					26h
UA=31
// Ukraine					26h
AE=31
// United Arab Emirates		26h
YE=31
// Yemen					26h
ZW=31
// Zimbabwe					26h
BD=31
// Bangladesh				26h
KH=31
// Cambodia					26h
CN=53
// China					48h
HK=31
// Hong Kong				26h
IN=52
// India					47h
ID=31
// Indonesia				26h
KR=33
// South Korea				28h
MY=52
// Malaysia					47h
PK=56
// Pakistan					51h
PH=31
// Philippines				26h
SG=52
// Singapore				47h
LK=31
// Sri Lanka				26h
TW=44
// Taiwan					39h
TH=31
// Thailand					26h
VN=31
// Vietnam					26h
AU=50
// Australia				45h
NZ=50
// New Zealand				45h
PG=31
// Papua New Guinea			26h
CA=39
// Canada					34h
JP=32
// Japan- Tele				27h
JM=56
// Jamaica					51h
TT=47
// Trinidad & Tobago		42h
TN=52
// Tunisia					47h
AL=31
// Albania					26h
AS=39
// American Samoa			34h
AD=31
// Andorra					26h
AO=31
// Angola					26h
AI=31
// Anguilla(UK)				26h
AQ=31
// Antarctica				26h
AG=35
// Antigua & Barbuda		30h
AM=39
// Armenia					34h
AW=39
// Aruba					34h

[Country_Not_Support_5G]
// =============================================================================
// WirelessMode 		code
// IEEE 802.11a         1
// IEEE 802.11b         2
// IEEE 802.11b/g       4
// IEEE 802.11b/g/n     16
// IEEE 802.11a/n       32
// =============================================================================
// [country code] = [default wireless mode]
ID=16
// Indonesia	
EG=16
// Egypt
IQ=16
// Iraq
KZ=16
// Kazakhstan
NA=16
// Namibia
RU=16
// Russian
UA=16
// Ukraine
BY=16
// Belarus
SY=16
// Syria
MD=16
// Moldova
MN=16
// Mongolia
TM=16
// Turkmenistan
UZ=16
// Uzbekistan

